Waterproof Brushed 60A Electronic Speed Controller ESC 1060 for RC 1/10 Car

Features

100% brand new and high quality

Water-proof and dust-proof, suitable for all-weather condition races.

Compact size, suitable for various car chassis.

Small size with built-in capacitor module.

Fwd/Rev/Br running mode fits for various vehicles (Fwd =Forward, Br=Brake, Rev=Reverse).

Great current endurance capability.

Great built-in BEC output capacity.

Automatic throttle range calibration, easy to use.

Easy to set the ESC parameters with jumpers.

Multiple protections: Low voltage cut-off protection for battery / Over-heat protection / Throttle signal loss protection.

Excellent operating feelings and plentiful adjustment options, suitable for most kinds of competitions.

Specifications:

Model: 1060-BRUSHED

Fwd. Cont. / Peak Current: 60A /360A

Rev. Cont. / Peak Current: 30A /180A

Voltage Range: 2-3S Lipo or 5-9 NiMH

Cars Applicable: 1/10: Touring Car, Buggy, Short Course Truck, Monster, Truggy, Rock Crawler and Tank

Motor Limit:

2S Lipo or 6 NiMH

540 or 550 Size Motor: ≥12T Or RPM<30000 @7.2V

3S Lipo or 9 NiMH

540 or 550 Size Motor: ≥18T Or RPM< 20000 @7.2V

4S Lipo or 12 NiMH

Not Available

Resistance: Fwd 0.001Ω, Rev 0.002Ω

BEC Output: 2A/5V (Linear Mode)

PWM Frequency: 1KHz

Dimension / Weight: 36.5\*32\*18 / 39g

Cooling Fan: Without cooling fan

Running Modes: Forward/Reverse/Brake, Forward/Brake, Forward/Reverse

Net Weight: 122g

Package includes:

1 x 1060-BRUSHED ESC