2015 NITECORE D2 Digicharger For 18650 14500 18350 Li-ion & Ni-MH +car charger US

Nitecore D2 Digicharger LCD Display Battery Charger Original Nitecore Charger 26650 18650 charger US

NEW 2015 VERSION NITECORE D2 Digicharger For 18650 14500 18350 Li-ion & Ni-MH US

Original Nitecore D2 Digcharger Battery Charger LCD Display Nitecore Charger for 26650 18650 18350 16340 14500 10440 US

NITECORE D2 Battery Charger Digicharger For 18650 Li-ion Ni-MH Ni-CD AA AAA US

**Features**

• Capable of charging 2 batteries simultaneously

• Each of the four battery slots monitors and charges independe ntly

• Compatible with and identifies Li-ion (26650, 22650, 18650, 1 7670, 18490, 17500, 18350, 16340(RCR123), 14500, 10440), Ni-MH and Ni-Cd (AA, AAA, AAAA, C) rechargeable batteries

• Optimized charging design for IMR batteries

• Integrated LCD panel clearly displays charging parameters and progress

• Two conveniently located side buttons allow easy selection of specific battery types and charging parameters

• Intelligent circuitry detects the battery type and status bef ore entering automatic charge mode (CC, CV, dV/dt)

• Automatically detects battery power status and selects the appropriate voltage and charge mode (with the exception of LiFePO4 batteries which require manual selection)

• Compatible with LiFePO4 batteries

• Compatible with small capacity batteries

• Automatically stops charging when complete

• Features over-charge prevention to protect batteries

• Features temperature monitoring to prevent overheating

• Made from durable ABS (fire retardant / flame resistant)

• Features reverse polarity protection

• Designed for optimal heat dissipation

• Certified by RoHS, CE, FCC, CEC and KC

• Insured worldwide by Ping An Insurance (Group) Company of China, Ltd.

**Specifications**

Input: AC 100-240V 50/60Hz 0.35A(MAX), DC 12V 1A

Output voltage: 4.2V ±1% / 3.7V ±1% / 1.48V ±1%

Output current: 500mA x 2

Compatible with:

Li-ion / IMR / LiFePO4: 26650, 22650, 18650, 17670, 18490, 1750 0,

18350, 16340 (RCR123), 14500, 10440

Ni-MH / Ni-Cd: AA, AAA, AAAA, C

Dimensions: 143mm× 74mm×36mm

Weight: 168g (without batteries and power cord)

**Package:**

Nitecore D2 Digicharger x1

AC power cord x 1

Manual x1