X8000 Dual Lens Car DVR 140° Camera GPS 2.0" Dash Cam G-sensor Video Recorder

HD Car Camcorder Dual Car DVR Twins Cam GPS Loop Recording Camera X8000 CA HF

Dual Lens Car Camera Two Lens Vehicle DVR Dash Recorder GPS G-sensor CA365 X8000

HD Car Camcorder Dual Cam w/ G-sensor Car Dvr Twins Carcam Gps Camera X8000

**Product characteristics:**  
\* The product, the latest dual-lens portable car camcorder of our company, can take dual-channel synchronous high-definition video.  
 \* The reasonably designed key functions facilitate the operation of users.  
 \*The dual lenses, perfect patented combination design with small size, rotary lens of 180 °, and A + level high-resolution day/night wide angle of 140 °, may take dynamic video photographing outside by one and inside by the other and also can take photographing outside or inside by both simultaneously, which is easier for video photographing with high resolution at various angles in different occasions.  
 \* The built-in low-noise high-definition photosensitive elements can capture high-definition pictures in darker occasions.  
 \* The built-in 3G-sensor automatic sensitive elements, which can feel the gravity charge of X axis, Y axis and Z axis simultaneously in running, can record emergent events automatically. Covered to keep a complete event video file.  
 \* Support the function of GPS external active module which can record the running states, such as running time, speed, running direction and location. Using the special playing software attached to this product can help you examine the whole running track of the car.  
 \* Support high-definition photographing: 1280x480 30FPS (2CH Record), 640x480 30FPS (1CH Record).  
 \* The most advanced M-JPEG CODEC mode makes the video much clearer and more perfect.  
 \* The circulatory recording function can automatically delete the old and shoot the new.  
 \* The seamless recording may ensure the event is recorded completely without skip.  
 \* The password protection makes other people cannot access and check the files except the owner.   
 \* The automatic time/date watermark may ensure when the event is recorded accurately.  
 \* The startup delayer may prevent pulse current damaging the camera in starting the car.  
 \* The automatic power-on I starting the car and power-off 30 seconds after killing the engine may ensure the event is recorded completely.  
 \* The anti-shake function may ensure the recorded event is clearer.  
 \* Support recording emergent event: in case of emergent event, the user presses the emergent event button and the video 60 seconds before and after pressing it will be captured, stored and not covered.  
 \* Support the audio ON/OFF function of video to satisfy the need of users.  
 \* Support the current of DV 12 to DV24, and it can be used for large vans, large trucks and buses.   
 \* Support the SDHC memory card with a large volume, even 32GB at most, and please choose 4GB Class 6 level above.  
 \* Support hot plug of SD memory card, plug out or in SD memory card under power-on state, and this product may not be powered off automatically.  
 \* Support CVBS output and playing videos on TV by attached special AV output cable.  
 \* The shortcut key for power down mode may turn off the screen for power saving at any time.  
 \* The built-in function of simultaneously charging and taping.  
 \* The built-in microphone/loudspeaker and dual-channel stereo output brings better sound effect.   
 \* Authenticated by international safety regulations like Taiwanese BSMI, CE and FCC, this product is manufactured in a lead-free process of RoHS, which is our wish to love the earth and protect the environment with you.  
  
**Product Specification:**  
Size of LCD screen :2.0 inch high-definition TFT-LCD (960\*240 Pixel)   
Lens :Dual lenses of 140 degree A + wide angle   
Sensor : CMOS   
Language :English, Chinese, Japanese, Russian   
Resolution :1280x480 30FPS (2CH Record), 640x480 (1CH Record)   
Format of image :M-JPEG(AVI)  
Loop recording : Support   
No Seam record : Support   
Emergent event key :Support   
Audio switch :Support   
Image flip : Support   
G-SENSOR : Internal   
GPS :Support external GPS   
Memory :Micro SD up to 32GB, at least above 4GB, and access speed of Class 6 above (The card is not included )   
Audio :Built-in stereo microphone and loudspeaker   
Encryption function : Support   
Muting switch : Support   
Video signal : PAL/NTSC   
Video output : CVBS   
AV out :Support   
Time/Date setting:Support   
Time/Date watermark:Support   
Battery : Polymer Li-ion Battery 700Mah/3.7V   
Operating system :WIN7/Windows 2000/XP/Vista   
Operating temperature:-10°~60 °  
Storing temperature :-20°~70°  
Weight of machine :95g   
Size of machine :135(L) x 24(H) x 52(W)mm

**Package including:**  
1 x X8000 HD Car DVR Camcorder Recorder GPS G-Sensor  
1 x Mount  
1 x English Manual  
1 x USB Cable   
1 x Car Charger