New XTAR VP2 LED battery charger (18650 / 14500 / 16340 / 18350 / 18500 / 26650)

 XTAR VP2 Charger XTAR VP2 with USB Output and LCD Screen Multi-function Charger

XTAR VP2 battery charger apply for 10440/14500/14650/16340/17670/18350/18500/18650/18700/22650/25500/26650

New XTAR VP2 LED battery charger (18650 / 14500 / 16340 / 18350 / 18500 / 26650)

**Features:**
1. Three charging current options (0.25A/0.5A/1.0A)
2. Three charging voltage options (3.2V/3.6V/3.8V)
3.Chargefor10440/14500/14650/16340/17670/18350/18500/18650/18700/22650/25500/26650 3.0/3.2V, 3.6V/3.7V, 3.8V Li-ion batteries
4. Low-Voltage, over-load and over-heat protection, power indication, stop supplying when low power
5. LED status indications
6. Real-time status display
7.Adopts PWM technology to control the high efficiency DC-DC circuit, lower the voltage and reduce energy loss
8. Three-stage charging and 0V battery activation
9. USB Output （5.0V/1.0A）
10. Adopts IC temperature monitor, avoid over heat
11. Small charge current when start to charge
12. Compact size, portable
13. Reverse-polarity and short circuit protection circuit
Input: 12.0V DC/1.0A
Charge current options:
0.25A CC Current: 250±30mA
0.5A CC Current: 500±50mA
1.0A CC Current: 1000±80mA
Corresponding termination voltage for three voltage options
3.2V: 3.6±0.05V
3.6V: 4.2±0.05V
3.8V: 4.35±0.05V

TC of 0.25A/0.5A: ≦50mA
TC of 1.0A: ≦80mA
Restart Charge automatically
3.2V Voltage Gear: 3.3±0.15V
3.6/3.8V Voltage Gear: 3.9±0.15V
Voltage Display Precision: ±0.03V
Operating Temperature: 0-40℃
USB Out-put parameter:
USB Output Voltage: 5.0±0.3V
Max USB Out Current: 1000mA
Battery Over-discharge Protection Voltage: 3.0±0.2V

**Package Content:**

VP2 Charger, Adaptor, Car Adapter, Manual, Warranty Card