Nitecore EC20 CREE XM-L2 T6 LED 18650 Flashlight 960 Lumens&Holster

Explore LED Flashlight 520 Hours Maximum Runtime Nitecore EC20 CREE XM-L2 T6

**Specification:**

Maximum output of up to 960 lumens

Integrated “Precision Digital Optics Technology” provides extreme reflector performance

Boasts a peak beam intensity of 12,450 cd and a throw distance of up to 222 meters

Innovative single button offers access to seven brightness levels and modes.

High efficiency constant current circuit board provides max runtime of 520 hours.

Integrated power indicator light displays remaining battery power (patented)

Power indicator’s secondary function displays battery voltage (accurate to 0.1V)

Instant access to ultra-low output Reverse polarity protection prevents damage from incorrectly inserted batteries

Constructed from aero grade aluminum alloy with HAIII military grade hard-anodized finish

Waterproof in accordance to IPX-8 (two meters submersible)

Impact resistant to 1.5 meters

Tail stand capability

**Dimensions**

Length: 128mm (5”)

Head diameter: 25.4mm (1”)

Tube diameter: 25.4mm (1”)

Weight: 76g (2.68oz)(without battery)

**Accessories**

Quality lanyard, spare O-ring,Holster