H.264 1.0 MP HD 720P P2P Pan/Tilt WiFi Wireless SD IR Network IP Security Camera

Wireless WiFi H.264 1.0 MP HD 720P P2P Pan/Tilt SD IR Network IP Security Camera

[Wireless Pan Tilt Security Network CCTV IP Camera NightVision WIFI indoor](http://www.ebay.com/itm/Wireless-Pan-Tilt-Security-Network-CCTV-IP-Camera-NightVision-WIFI-Webcam-indoor-/121590194495?pt=LH_DefaultDomain_0&hash=item1c4f57213f)

720P Wireless WIFI indoor NightVision Pan Tilt Security Network CCTV IP Camera

**Description**

H.264 1/4" Color CMOS Sensor, 1.0MP

Support 1, 4 and 9Ch image display and full screen view on web browser

Support QR Code Scanning.

Support maximum 32GTF Card

High image & video quality. Two-way audio monitoring

P2P(Plug&Play)technology, penetration degree can be 99%

Allow remote Pan/Tilt control (Pan:350°& Tilt:120°)

Mechanical IR-Cut device offers outstanding day/night performance, great color;

Mobile Monitor: iPhone(APP Store), Android

(1280\*720) Pixels 720P/D1/VGA/QVGA/QCIF, dual stream

Allow remote viewing & record from anywhere anytime

Wi-Fi compliant with wireless standards IEEE 802.11b/g/n

Support TCP/IP, ONVIF, RTSP, P2P SMTP, HTTP, FTP, PPPoE and other Internet related protocols;

**Specification**：

System security:Account, password authority management

Free DDNS: Free DDNS, supports dynamic IP.

View by phone:Support HD pic IOS, Android mobile view (iOS 4.3、Android OS 2.3 above)

Local Storage: support up to 32GB MicroSD card ，24-hour loop recording.

Monitor Advantage : Support PC computer monitoring, Smartphone multi-pic view.

**PnP:**

Plug & Play,99% penetration rate, Easy to setup:

1. connect the network cable and power adapter

2.install APP, scan UID code to add camera.

3.Click online camera to view the camera.

QR Code Scanning: UID scan technology applied, easy to operate, and highly confidential.

Super Client: 1,4,9,16,25,36, 64,81-channel central management software, no user number limitation ,centralized surveillance, remote record and playback, alarm email ect.

**System**

OS:P Embedded Linux OS

Control protocol: ONVIF 2.0 protocol, high interoperability

Video coding Multi stream：720P@30fps+VGA@30fps+QVGA@30fps+720P @1fsJPEG capture

Bit Rate: CBR/VBR, output bit rate range：128～4096kbps

Processor : Hi processor, built in ARM926 @Max. 440MHz and high-speed video co-processor

**Video**

Compression Format: H.264 baseline profile@levels:3.1/Motion-JPEG

Frame rate: 30fps/24fps（720p）

Resolution: 720P(1280\*720), VGA(640\*480), QVGA(320\*240)

Sensor: 1/4 720p Progressive CMOS sensor

Minimum illumination: 0.8Lux/F1.４（colorful model ）,0.3Lux/F1.（B&W mode）

SNR: ≥39dB

IR control IR turned on: night vision view enabled, infrared Ray, ICR auto detect.IR turned off:

night vision disabled, infrared ray off, ICR stay in day view mode.

Electronic shutter: 1/50s(1/60s）-1/100, 000s

CMOS: support AWB, AGC, BLC

Lens/viewing angle : 3.6mm@F1.４/56.14˚

**Night Vision**

Night vision: Dual IR-CUT Filter auto switch, 12pcs 850nmΦ5mm LED,10m IR distance

Compression format: ADPCM/32kbps

Input: 1 Channel Line in (3.5mm phone jack) &1 Channel Internal -48dB **Microphone**

Output:1 Channel Line out (3.5mm phone jack)&Internal speaker(8Ω1W)

Network P/T Pan:355°,Tilt:120°

Preset Position: support up to 15 preset positions

network interface: 10Base-T/100Base-TX Ethernet interface

Network Protocol: TCP/IP, HTTP, TCP, UDP, SMTP, FTP, DHCP, DNS, DDNS, NTP, UPnP, RTSP, P2P, etc.

wireless network security: WPS encryption

Online visitor: Support 4 online visitors simultaneously

IP address: Dynamic IP and static IP address

WIFI 802.11 b/g/n

housing material: engineering plastics

Application environment: Indoor

Rated Voltage: DC5±0.3V

Temperature: -10~50 °C

**Power consumption**

rated power：3.5W (IR opening )/maximum power：7W(P/T working )

Package size: 200×179×123mm (L×W×H)

**Accessories**

Power adapter, user manual, warranty card, mounting bracket, screws.

Alarm

Motion Detection: Support motion detecting

System Requirement

System configuration: Win98 SE/ME/2000/XP,Vista,iPhone iOS4.3,The android version 2.3 or higher

**Package included**

1 \* IP Camera

1 \* Adapter

1 \*user manual

1 \*Bracket

1\*CD

1\*Wireless