CCTV Wireless Wifi 720P HD H.264 P2P 1MP IP Network Home IR Security Camera P/T

 720P Wireless WIFI CCTV Security Network IP Camera Day/Night Indoor HD

Wireless Pan Tilt 720P Security Network CCTV IP Camera Night Vision WIFI

720P Wireless Pan Tilt Security Network CCTV IP Camera Night Vision WIFI

Night Vision WIFI Wireless Pan Tilt 720P Security Network CCTV IP Camera

**Description**

H.264 1/4" Color CMOS Sensor, 1.0MP

Support 1, 4 and 9Ch image display and full screen view on web browser

Support QR Code Scanning.

Support maximum 32GTF Card

High image & video quality. Two-way audio monitoring

P2P(Plug&Play)technology, penetration degree can be 99%

Allow remote Pan/Tilt control (Pan:350°& Tilt:120°)

Mechanical IR-Cut device offers outstanding day/night performance, great color;

Mobile Monitor: iPhone(APP Store), Android

(1280\*720) Pixels 720P/D1/VGA/QVGA/QCIF, dual stream

Allow remote viewing & record from anywhere anytime

Wi-Fi compliant with wireless standards IEEE 802.11b/g/n

Support TCP/IP, ONVIF, RTSP, P2P SMTP, HTTP, FTP, PPPoE and other Internet related protocols;

**Specification**：

System security:Account, password authority management

Free DDNS: Free DDNS, supports dynamic IP.

View by phone:Support HD pic IOS, Android mobile view (iOS 4.3、Android OS 2.3 above)

Local Storage: support up to 32GB MicroSD card ，24-hour loop recording.

Monitor Advantage : Support PC computer monitoring, Smartphone multi-pic view.

**PnP:**

Plug & Play,99% penetration rate, Easy to setup:

1. connect the network cable and power adapter

2.install APP, scan UID code to add camera.

3.Click online camera to view the camera.

QR Code Scanning: UID scan technology applied, easy to operate, and highly confidential.

Super Client: 1,4,9,16,25,36, 64,81-channel central management software, no user number limitation ,centralized surveillance, remote record and playback, alarm email ect.

**System**

OS:P Embedded Linux OS

Control protocol: ONVIF 2.0 protocol, high interoperability

Video coding Multi stream：720P@30fps+VGA@30fps+QVGA@30fps+720P @1fsJPEG capture

Bit Rate: CBR/VBR, output bit rate range：128～4096kbps

Processor : Hi processor, built in ARM926 @Max. 440MHz and high-speed video co-processor

**Video**

Compression Format: H.264 baseline profile@levels:3.1/Motion-JPEG

Frame rate: 30fps/24fps（720p）

Resolution: 720P(1280\*720), VGA(640\*480), QVGA(320\*240)

Sensor: 1/4 720p Progressive CMOS sensor

Minimum illumination: 0.8Lux/F1.４（colorful model ）,0.3Lux/F1.（B&W mode）

SNR: ≥39dB

IR control IR turned on: night vision view enabled, infrared Ray, ICR auto detect.IR turned off:

night vision disabled, infrared ray off, ICR stay in day view mode.

Electronic shutter: 1/50s(1/60s）-1/100, 000s

CMOS: support AWB, AGC, BLC

Lens/viewing angle : 3.6mm@F1.４/56.14˚

**Night Vision**

Night vision: Dual IR-CUT Filter auto switch, 12pcs 850nmΦ5mm LED,10m IR distance

Compression format: ADPCM/32kbps

Input: 1 Channel Line in (3.5mm phone jack) &1 Channel Internal -48dB **Microphone**

Output:1 Channel Line out (3.5mm phone jack)&Internal speaker(8Ω1W)

Network P/T Pan:355°,Tilt:120°

Preset Position: support up to 15 preset positions

network interface: 10Base-T/100Base-TX Ethernet interface

Network Protocol: TCP/IP, HTTP, TCP, UDP, SMTP, FTP, DHCP, DNS, DDNS, NTP, UPnP, RTSP, P2P, etc.

wireless network security: WPS encryption

Online visitor: Support 4 online visitors simultaneously

IP address: Dynamic IP and static IP address

WIFI 802.11 b/g/n

housing material: engineering plastics

Application environment: Indoor

Rated Voltage: DC5±0.3V

Temperature: -10~50 °C

**Power consumption**

rated power：3.5W (IR opening )/maximum power：7W(P/T working )

Package size: 200×179×123mm (L×W×H)

**Accessories**

Power adapter, user manual, warranty card, mounting bracket, screws.

Alarm

Motion Detection: Support motion detecting

System Requirement

System configuration: Win98 SE/ME/2000/XP,Vista,iPhone iOS4.3,The android version 2.3 or higher

**Package included**

1 \* IP Camera

1 \* Adapter

1 \*user manual

1 \*Bracket

1\*CD

1\*Wireless