Wireless Serial 4 Pin Bluetooth RF Transceiver Module HC-06 RS232 With backplane

Specification:

Works with any usb Bluetooth adapter

Default baud rate:9600,8,1,n

Built in antenna

Coverage up to 30ft

Bluetooth version: V2.0+EDR

Operating voltage: 3.3V

Default baud rate: 9600,8,1,n

Signal coverage: 30ft

Cable length: 21.5cm

Features:

Commeracial series: Bluetooth module board series

With LED indicator light, use 150ma and 3.3v regulation chip

With VCC, GND, TXD, RXD foot for the Bluetooth

With “ Re-seach” button(on/off/wake foot for it , external MCU outinput: high level” can control module to research)

Compatible with Bluetooth master module”slave module” or master slave module

Input voltage: 3.3~6V

Package list:

1 x HC-06 RS232 Module