New RX LCD 5802 5.8GHz LCD Diversity Receiver 7 Inch Monitor Built-in Battery

Features:

Built-in Dual Receiver Automatically for best reception Automatic Antenna Switching

Dual buffered AV outputs

Can receive 2 different channels at the same time

Not affect by 2.4GHz R/C Radios

AV Receiver with Diversity inputs

Small, light weight, durable

4 Bands and total 32 Channels

Built-in battery , easy to carry and outdoor use

A key to automatic signal search,Simple operation

Work status OSD display:Always be aware of the device working condition.

Specifications:

Built-in 5.8Ghz Dual diversity receiver automatically for best reception

Built-in 2CH 5.8Ghz AV output and 1CH AV input

Built-in high performance Li-POLYMER Battery: 2450mAH/7.4V

Work status OSD display : RSSI indication ; Battery indicator;Channel indication

A key to automatic signal search

Support Chinese and English menu

Screen size:7''

Screen type:TFT LCD Screen/long life, LED backlight

Resolution: 800\*480

Brightness: 450cd/m2

View Angle:140/120degree (Horizontal/Vertical)

Size:180mm x 120mm x 50mm(Note:Sunshield height:28mm)

Working Voltage: DC 7~16V

Power Consumption: 650 mA @12V

Battery charging current : 850mA @12V ( max )

Working temperature: -10C~+ 65C

Connectors:SMA female(outer hole)

Antennas Connectors:SMA male (inner needle)

Package includes:

1 x 7'' LCD Screen Receiver Monitor with built in Rechargable Battery

2 x 5.8G Antenna

2 x AV Cable

1 x Charging Cable

1 x Shade Hood