R3000 G-sensor GPS Dual Lens HD2.7" Car DVR Auto Crash CAM Camera Video Recorder

G-sensor 2.7" Car DVR Dual Lens Vehicle Camera Video Recorder Dash Cam G-sensor HDMI

2.7" 140 Degree Wide Angle Dual Lens Car DVR Camera Recorder Motion Detection Night Vision G-Sensor

New 2.7" Dual Lens Car DVR Vehicle Camera Video Recorder Dash Cam 140 degrees

**Features:**  
Ultra small volume;

The front lens with ultra wide angle of 140 degrees can be rotated up and down 20 degrees;

The back lens with ultra wide-angle of 120 degrees high resolution;

This perfect modular design is more convenient for various angle and high resolution video shooting.

Built-in 1/4 inch low-noise and high-quality photographic element can capture ultra clear picture in a dark place.

Built-in lithium battery with charging and meanwhile recording function.

Built-in microphone/speaker.

Support high-capacity Micro TF Card(Not Included)

Automotive turning on and recording function when the vehicle start.

With a delayed start function to prevent transient pulse current damage machine at the moment the vehicle start.

GPS scanning and positioning。

Gravity induced SENSOR  
  
**Specifications:**  
· LCD screen size: 2.7"（16: 9）

· Lens: Front lens with ultra wide angle of 140 degrees; back lens with ultra wide-angle of 120 degrees Optional

· language: English / German / French / Spanish / Italian / Portuguese /Traditional Chinese / Simplified Chinese/ Japanese

· Video format: AVI

· TF memory card slot: Micro TF

· Microphone / speaker: Built-in

· Television output: NTSC/PALTV

· Output and DC access: 5V 500MA

· Battery: Built-in lithium polymer battery

· System requirement: Windows 2000/XP/Vista/Windows 7,MAC OS x above 10.3.6

**Package Content:**  
1 x 2.7" Dual lens DVR·

1 x Car Charger·

1 x GPS module·

1 x Mount

1 x User manual