LCD Universal Battery Power Charger For 14500 18350 18650 26650 AA AAA C US Plug

Soshine H4 4 slots Intelligent Lithium LCD Display Battery Charger For 18650 26650 16340 Li-ion / AA AAA Ni-MH NIMH / LiFePO4 US Plug

Soshine H4 4 slots Intelligent Lithium LCD Display Battery Charger For 18650 26650 Li-ion / AA AAA Ni-MH / LiFePO4 +power supply US Plug

Soshine H4 LCD Universal Battery Charger for Li-ion / Ni-MH / LiFePO4 Batteries US Plug

**Specifications:**

Model: Soshine H4

**Features:**
- Automatic 3.7V/1.2V battery cell voltage and polarity detection
- Mix charge the battery, reverse protection, precision end-of-charge voltage detection
- Over charging timeout protection
- LCD displays for multi-information, battery type, voltage, time, charging percentage, charging capacity
- Auto alert indication for worse battery cell and bad battery cell

**Charger:**
- For Ni-MH batteries: put into the battery, the charger automatically identifies and directly charge. The default charging current is 500mA. If you want to choose a differnt charging current, please choose 1000mA/ 500mA before putting into the battery, then press the Enter key and put into the battery.
- For Li-ion/ LiFePO4 batteries: Before putting into the battery, adjust the left and right buttons to select the channel which will charge the battery. Up and down buttons to select the battery type. Press the Enter key to confirm. Continue to select the charge current, 1000 mA/ 500 mA/ 250mA, and then press the Enter key to confirm.

DC In: 12V 2000mA/ 12V > 24W(Photovoltaic solar panel)

Output: 250/ 500/ 1000mA\*4 @ Lion 3.7V battery/ @ Ni-MH 1.2V battery/ @ LiFePO4 3.2V battery

Charge Mode: CC/ CV(Li-ion battery/ LiFePO4 battery)/ DELTA V(Ni-MH battery)

**Package Include:**

1 x Charger

1 x Adapter

1 x Car charger