2015 Nitecore P12 1000 Lumens Tactical Cree XM-L2 Flashlight+2600mAh 18650 Battery

Nitecore 18650 520 Hours Maximum Runtime XM-L2 LED Flashlight P12 1000 Lumens+2600mAh 18650 Battery

Portable Explore Flashlight 520 Hours Maximum Runtime Nitecore P12 1000Lumens 18650+2600mAh 18650 Battery

**Features**• Premium CREE XM-L2 (T6) LED  
• Maximum output of 950 lumens  
• Second generation ‘Crystal Coating Technology’ combined with ‘Precision Digital Optics Technology’ provide extreme reflector performance  
• Boasts a peak beam intensity of 12,450cd and a throw distance of up to 222 meters  
• High efficiency circuit board provides up to 520 hours runtime on low  
• Side switch interface provides one-handed operation and easy access to all functions  
• Side switch features an indicator light which displays remain ing battery power (patented)  
• Power indicator ’s secondary function displays battery voltage (accurate to 0.1V)  
• Intelligent memory function stores preferred brightness setting  
• High-efficiency regulation circuit provides unwavering output  
• Toughened ultra-clear mineral glass with anti-reflective coating  
• Constructed from aero grade aluminium alloy with HAIII military grade hard-anodized finish  
• Waterproof in accordance with IPX-8 (two meters submersible)  
• Impact resistant to 1.5 meters  
• Stainless steel titanium-plated clip included  
• Tail stand capability  
  
**Dimensions**  
Length: 139mm (5.47”)  
Head Diameter: 25.4mm (1”)  
Tail Diameter: 25.4mm (1”)  
Weight: 88grams (3.10oz)(without battery)  
  
**Accessories**  
Quality holster, clip, tactical ring, lanyard, spare tail cap, spare O-ring

**Package Include:**

1\*P12 flashlight

1\*NL186(2600mAh 18650 battery)