720P 1.0 MP HD H.264 Wireless WIFI PTZ IR Cut Indoor IP Security Camera

5V Wireless WIFI HD 720P IP Camera ONVIF In/Outdoor Security Day/Night Vision

Wireless Wifi CCTV 720P HD H.264 P2P IP Network Home IR Cut Security Camera P/T

Security Night Vision 720P WiFi Outdoor Waterproof Wireless IR Network IP Camera

**Key Features**

720P HD Indoor Wireless IP Camera

Built-in 1/4 Inch 1.0 Megapixel CMOS

Built-in 3.6mm Fixed Lens

Support IR-CUT,10pcs LEDs and 10M IR Range

Support 1MP:1280\*720,VGA,QVGA

Support Multi-Screen Software and CMS

Support P2P,Two-way Audio and 32GB TF Card Storage

Support iPhone,iPad,Android Smartphone Monitoring

Support up to 4 Users Online Simultaneously

**Specifications**

Style : PTZ

Sensor:CMOS

Sensor Size:1/4 Inch Color CMOS Sensor

Resolution:1.0 Megapixels

Lens (mm) : 3.6mm

Viewing Angle (Degree) : 75 Degrees

Minimum Illumination (Lux) : 0.1 LUX

**Video Image/Audio Setting**

Compression: H.264

Video Frame Rate (FPS): 30fps

Refresh Rate: Outdoor, 60HZ, 50HZ

Video Adjustment: Auto White Balance, Contrast Adjustable, Brightness Adjustable, Auto Backlight Compensation

OSD:Yes

Audio Output: External Speaker

Audio Input: External Mic

Audio Compression Standard ADPCM

**Communication&Interface**

Network Interface :Wi-Fi/802.11/b/g, RJ-45 10/100Mb self-adaptable Ethernet slot

Supported Protocol DNS, FTP, PPPoE, UPNP, DDNS, HTTP, SMTP, DHCP, TCP/IP

Wireless Security: WPA2, WPA, WEP

IP Mode: Static IP address, Dynamic IP address

Maximum SD Card Support (GB): 32GB

DDNS (Free): Yes

Alarm Action: Email Photo, FTP Photo

**Physical/Environment**

Environment: Indoor

Power Supply (V): DC 5V

Power Consumption (W) :6W

Operate Temperature (℃): 0-55 Degree Celcius

Storage Temperature (℃): -10-60 Degree Celcius

Humidity (%) RH: 20%-85%

Size (L x H x W, mm): 200 x 179x 123m

**System Requirment**

Supported Mobile Systems： Android, Windows Mobile, Symbian, iPhone OS

Supported Operating Systems: Mac os, Microsoft Windows 7, Microsoft Windows Vista, Microsoft Windows XP, Microsoft Windows 2000, Microsoft Windows ME, Microsoft Windows 98

Supported Browers Other Standard Browser, Google Chrome, Firefox, Safari, IE

Client Software: Yes

**Additional Features**

Features Plug and play, IR-cut, Remote Access, Motion Detection, Day Night

HDD Recording Function :Yes

IR Night Vision Distance (m): 10 Meters

Two-way Radio: Yes

User Account Setting (Level): Three Levels

Online User: 4

Update Firmware: Yes

Pan/Tilt-Horizontal (Degree): 355 Degrees

Pan/Tilt-Vertical (Degree): 120 Degrees

Language :English, Simplified Chinese

**What's in the box?**

1\*IP camera

1\*Bracket

1\*CD

1\* Power adaptor

1\*Wireless

1\*User Manual