Wireless P2P IP Pan/Tilt/Night Vision Network Camera Audio Cam Security Moniter

Night Vision P2P Wireless IP/Network Camera Audio Cam Security Moniter

[Wireless Pan Tilt Security Network CCTV IP Camera NightVision WIFI Webcam indoor](http://www.ebay.com/itm/Wireless-Pan-Tilt-Security-Network-CCTV-IP-Camera-NightVision-WIFI-Webcam-indoor-/121593894230?pt=LH_DefaultDomain_0&hash=item1c4f8f9556)

Indoor Night Vision WIFI Webcam Wireless Pan Tilt Security Network CCTV IP Camera

**Product Introduction:**

This Wireless IP Security Network Pan Tilt Camera features a high quality video sensor combined with pan, tilt, and remote internet viewing. In addition, the camera supports motion detection as well as a built in network video recording system. It is smartphone compatible (iOS and Android) and accessible over the internet using standard browsers (Internet Explorer, Safari, Firefox & Chrome). The camera functions well as an iPhone baby monitor, granny camera, dome camera, hidden camera, PTZ camera, or as part of a home or office security system with remote internet monitoring ability.

 **Product Feature:**

* WiFi: Wireless network connection. No complicated wiring
* Infrared Night Vision: Automatically turn on in low light and in darkness
* Mobile Devices: Support remote viewing on mobile devices. iPhone/iPad/Android OS supported
* Two-way Audio: Communicate with family and friends on mobile devices. Talk to camera or listen to camera.
* Pan/Tilt Control: Move the camera as you desired. Pan horizontally up to 340 degrees, tilt vertically up to 90 degrees
* Motion Detection: Automatically detect moving objects and trigger alarm.Send alert emails to user and upload screen captures to FTP server
* Power adapter cord extended to 5ft
* Enhanced WiFi signal reception, WiFi IEEE 802.11b/gg
* Enhanced camera shell rigidity

**Product Specification:**

* Image sensor: 1/4" color CMOS
* Lens: 3.6 mm
* Infrared LED: 10 PCS
* Pixel: 300,000
* Night vision distance: 10M (32 feet)
* AWS/AGC/AES/ exposure: Auto
* Min. Illumine: 0.1 Lux
* Audio: 2- way audio
* Input: Built-in microphone
* Output: Built-in speaker
* Compression: MJPEG
* Max. frame rate: 30 fps
* Resolution: 640 x 480, 320 x 240, 160 x 120
* PT angle: Horizontal 340 degree; vertical 90 degree
* Wi-Fi: IEEE 802.11b/g
* Network interface: RJ-45 (10BASE-T/100BASE-TX)
* Motion detection: 5 levels sensitivity
* Alarm events: Notification (snapshots) via email or FTP ,Video recording to Windows PC
* Periodic sending : Send pictures to Email/FTP within preset schedule
* Web browser: IE 6.0 or above version, Chrome, Firefox, Safari, Opera, etc
* Simultaneous viewers: 6 viewers@320x240, 4 viewers@640x480, 6 viewers@160x120
* Mobile view: Support iOS and Android device
* Power: DC 5V, 1.5A
* Power consumption: 4W/6W (infrared off/on)
* Operating temperature: -10 to +50 C (+14 to +122 F)
* Operating humidity: 10-80%RH non-condensing

**Package Content:**

* 1x Wireless IP Camera
* 1x power adapter for Camera
* 1x Wi-Fi Antenna
* 1x CD
* 1x bracket
* Some Screws