IR LED ARRAY CCTV Security DVR Camera USB SD-Card Motion Detection Camera

Night vision IR LED ARRAY CCTV Security DVR Camera SD-Card Motion Detection Camera

SD-Card Motion Detection Camera CCTV IR LED ARRAY DVR Camera

[IR LED ARRAY CCTV Security USB DVR Camera Micro SD-Card Motion Detection Camera](http://www.ebay.com/itm/IR-LED-ARRAY-CCTV-Security-USB-DVR-Camera-Micro-SD-Card-Motion-Detection-Camera-/310638100521?pt=LH_DefaultDomain_0&hash=item4853794029)

**Features :**

This camera is a complete video monitoring system. It has functions of video recording, motion

detection, infrared monitoring at night time, photosensitive induction and circulating storage.

Simple operation, just plug into a wall power socket, it will auto start video recording,

24hrs x 7days standby

Using 3rd generation LED Array, makes the night vision more clearer, viewing angle more wider,

viewing distance more longer upto 30meters, lifetime more longer 3-5yrs

Smaller video size, using 3GP video format, video file size is smaller than avi or others

Two recording mode

1. Continuous recording with motion detection (Default mode) - if motions are

detected, it will record video at 12fps, if no motion detected, it will record video at 1fps

(it takes little memory only). The design like this is to gurantee all situations are recorded and

occupy less memory.

2. Motion detection only (optional, config by user or arrange before shipment)

- if motions are detected, it will start recording, if no motion detected, it will be in standy

mode, no recording.

Circular recording, when storage (Micro SD-card) is full, new video file will replace the first

one, second, third and so on, never worry about run out of storage. Files will be saved in 30mins

per file

Using external storage media, support Micro SD-card, video files are stored inside, Max. support

up to 32GB (recommend using good quality cards, and the machine does not include a card by default)

A 4GB Micro SD-card can store upto 24hrs video files - 3.6mm camera LEN by default, the viewing

angle is around 95 degree, 2.8mm camera is another option its viewing angle is 110 degree

To playback video, just take out the card plug it into computer (a card reader is included)

Item Dimension : 92mm/3.5" Diameter

Suitable for security surveillance at homes, schools, shops, shopping malls and factories and so on

Also good for used on Taxi or Bus for surveillance purpose

**Item Specification:**

Micro Processor : ARM9 32-bit Microprocessor core

Video Encoding : 3GP

Video Resolution : VGA 640x480/CIF 320x240 pixel

Signal system : Digital

S/N Ratio : 48db

White Balance : Auto

Camera Len : 3.6mm

HD Camera : 300,000 pixel high-definition 1/4" CMOS image sensor

Storage : Micro-SD card, max. support up to 32GB

Built-in microphone

Built-in 2pcs 3rd generation LED array (850nm wavelength)

Viewing at night distance is about 30 meters

Motion detection distance is 5 meters

Voltage : AC 110 ~ 220V, DC 5V 1A

**Package Content:**

1 x Motion Detection Dome Camera Video Recorder ( SD card not included)

1 x CD disk

1 x User manul

1 x TF-card reader

1 x Mounting screws