Mini RF LED Remote Controller Wireless Dimmer for 3528 5050 Strip Single Color

Specification:

Working Voltage: DC 5V-24V

Output current: 3 way, <4A (each channel)

Remote frequency: 433.92MHz

Remote distance: >15m

Max current : 12A

Max output power :144W

Working temperature:-30~+75 centigrade

Auto memorizefunction

Control Function:

Speed; Brightness; Color; Mode. 19 Dynamic Modes; 20 Static Colors

Package included:

1x RF Remote (include battery)

1x Controller