FT232RL 3.3V 5V FTDI USB to TTL Converter Adapter Module for Arduino Mini Port

Features:

FT232RL adapter module

Chip: FT232RL

USB supply power, can chose 5V or 3.3V interface level

PCB size: 17mm\*32.5mm

Elicit all signal port of FT232RL chip, TTL/CMOS level

RXD/TXD transceiver communication signals indicator light

If need other level, can provide target voltage on VCC and GND Pin directly

Package list:

1 x FT232RL 3.3V 5V FTDI USB to TTL Converter Adapter Module for Arduino Mini Port