Front Master Power Window Switch Driver Side Left LH for Ford F150 Truck Mercury

NEW Master Power Window Switch Driver Side Left LH for Ford Mercury F150

Front Master Power Window Switch Driver Side Left LH NEW for Ford Mercury

Power Master Window Switch Front LH Driver Side for Ford F150 Mercury

**Specifications:**

Fits LH (Driver Side) FRONT DOOR

Arrow Style switch which uses two down arrows for the auto down function

5 Button master switch

Auto down feature for left front window

On/Off switch to lock windows

Replaces dealer part number: 5L1Z-14529-AA, 5L1Z14529AA

Built to strict quality control standards

100% tested prior to leaving the factory

Fits 4 Door Models only

Note: For Crown Vic, Grand Marquis, and Marauder models there were two types of master switches used. One type says "AUTO" for the auto down feature. The other type uses two down arrows to signify the auto down feature. This switch is the arrow style that uses two down arrows. They will not interchange because of length differences.

**Brand NEW fitting for the following years and models:**

2002-06 Ford Crown Victoria Arrow Style Power Window Switch Front Driver Side

2007-08 Ford Crown Victoria Power Window Switch Front Driver Side

2003-06 Ford Expedition Power Window Switch Front Driver Side

2004 Ford F150 Truck New Body Style Power Window Switch Front Driver Side

2005-08 Ford F150 Truck Power Window Switch Front Driver Side

2006-08 Lincoln Mark LT Power Window Switch Front Driver Side

2006-08 Mercury Grand Marquis Power Window Switch Front Driver Side

2002-06 Mercury Grand Marquis Arrow Style Power Window Switch Front Driver Side

2003-04 Mercury Marauder Arrow Style Power Window Switch Front Driver Side